To program the Wireless Keyless Entry (model G6K) to the Skylink Garage Door Opener (EQ Series):

1. On the motor, press the “LEARN” button once and release. The yellow LED will be on.

2. Within 30 seconds, enter your [PIN], [#] and the assigned [door number, 1 or 2 or 3 or 4]. For example: if the PIN is still set to factory default, 0 0 0 0, and you only have one garage door, enter [0 0 0 0] [#] [1].

3. If the PIN is correct, the keypad will emit 3 beeps and the yellow LED on the motor will immediately turn off.

4. The G6K may now be used to operate the garage door.

Program the Wireless Keyless Entry (model G6K) to the Skylink Garage Door Opener (IQ Series):

1. Press and hold the PROG button on the LCD Wall Console for 10 seconds until the “PROG” icon appears on the display.

2. Press the PROG button again until the “remote” icon appears on the display.

3. Activate the keypad transmitter by entering the password and door number. For example, if the password is 0000 and door 1 is used, you should enter [0000][#][1]. If keypad is programmed, the “remote” icon will stay on.

Refer to the manual of the garage door receiver to erase the keypad transmitter.

G6K PIN Reset: 

1. Remove the batteries. 

2. Open the back T-shaped cover.

3. On the top of the circuit board, you will see a single black connector in a horizontal position. It will be on the left two pins (1-2). Move it to the two right pins (2-3).

4. Insert the batteries.

5. Enter [7 6 5 4 3 2 *]. The keypad will emit a long beep confirming reset. 

6. Move the black connector to its original position of 1-2. Do not touch any keys or change any settings for two hours.

7. After two hours the PIN will be back to factory default of 0 0 0 0.

Note: Remember to move the connector to its original position of 1-2. If left on 2-3, it will consume higher current and drain the batteries.

Keypad Operation:

You must always enter your [PIN], [#], and the assigned [door number, 1 or 2 or 3 or 4] to be able to operate the door. Solely entering your 4-6 digit PIN is not enough.  

To change PIN:

1. Enter your current PIN

2. Press *

3. Enter your new PIN (4-6 digits)

4. Press *

5. Enter your new PIN again

6. Press *

7. A long beep will confirm change

For example: Changing the factory default 0 0 0 0 to 1 2 3 4. Press 0 0 0 0 * 1 2 3 4 * 1 2 3 4 * - a long beep will be emitted.

Note: Do not press [#] and the assigned [door number, 1 or 2 or 3 or 4] during change PIN sequence. That is the command to operate the door.

Para programar el modelo G6K a el abridor de puerta de garaje (Skylink EQ Serie):

1. En el motor, presióne el botón de "APRENDIZAJE" una vez y suelta. La luz amarilla se encendera.

2. Dentro 30 segundos, entra el [CóDIGO], [#] y el [número de puerta]. Por ejemplo: si el código es 0 0 0 0, y sólo tiene una puerta de garaje, debe entrar [0 0 0 0] [#] [1].

3. Si el código es correcto, el teclado emitirá 3 sonidos y la luz amarilla del motor se apagará.

4. Ahora el teclado se puede utilizar para operar la puerta del garaje.

Para programar el modelo G6K a el abridor de puerta de garaje (Skylink IQ Serie):

1. Mantenga presionado el botón PROG en la consola de pared de LCD por 10 segundos hasta que el simbolo de "PROG" aparesca en la pantalla.
2. Presióne el botón PROG de nuevo hasta que el simbolo de "remoto" aparesca en la pantalla.
3. Activar el transmisor del teclado, entra el [CóDIGO], [#] y el [número de puerta]. Por ejemplo: si el código es 0 0 0 0, y sólo tiene una puerta de garaje, debe entrar [0 0 0 0] [#] [1]. Si el control remoto está programado, el simbolo de "remoto" se mantendrá prendido

Lea el manual del receptor de la puerta del garaje para borrar el transmisor del teclado.
Perdí mi código:
1. Saca las baterías.

2. Abre la cubierta que se encuentra en la parte de atrás.

3. En la parte superior de la placa de circuito, verá un conector negro en una posición horizontal. Estara en las dos clavijas a la izquierda (1-2). Muevelo a las dos clavijas a la derecha (2-3).

4. Inserte las baterías.

5. Entrar [ 7 6 5 4 3 2 * ]. El teclado emitirá un sonido largo como una confirmación.

6. Mueva el conector negro a su posición inicial de 1-2 (la izquierda). No toque ningun botón o cambie cualquier configuración por dos horas.

7. Después de dos horas, el código será 0 0 0 0.

Nota: Si dejas el conector en posición 2-3, las baterías se descargaran porque se consume más energía. Recuerda de poner el conector en su posición original de 1-2.

Operación del teclado:
Usted siempre debe entrar su [CóDIGO], [#] y el [número de puerta] para operar la puerta. Únicamente introduciendo su código de 4-6 dígitos no es suficiente.

Para cambiar el código:
1. Entra su código actual
2. Presióne estrella [ * ]
3. Entra su nuevo código 
4. Presióne estrella [ * ]
5. Entra su nuevo código otra vez (4-6 dígitos)
6. Presióne estrella [ * ]
7. Un sonido largo confirmará el cambio
Por ejemplo: cambiar 0 0 0 0 a 1 2 3 4. Presióne 0 0 0 0 * 1 2 3 4 * 1 2 3 4 * - un sonido largo será emitido.
Nota: No presióne [#] y el [número de puerta] durante el cambio de código. Ese es el comando para accionar la puerta.
